


|  |  |
| --- | --- |
| D:\Backup\桌面\微信图片_20220812151419.jpg微信图片_20220812151419Parameter | |
| Product Name | RL-95mm-ICRGB |
| Product size | Φ95mm\*180mm |
| The LED type | epistar |
| The LED Quantity | 7 PCS |
| The beam Angle | 120° |
| The input voltage | DC24V |
| Color | RGB addressable |
| The IP rating | IP65 |
| Rated power | 2W |
| Regular line length | 180mm |
| Product appearance | Ball shape |
| Lamp lifetime | ≥50000 hour |
| Working temperature | -40℃~60℃ |
| Control | Dmx512 /SPI optional |

Product Advantages

Flreproof

Grade

V-0

Protect Grade

lP65

1. The appearance is exquisite and compact, and the spinning cone setting can effectively control the width of the lamps.

2. The bottom shell is made of flame-retardant ABS material, which is resistant to high temperature, and the light-transmitting surface is a UV-resistant and high-transmitting PC lampshade.

3. The light source adopts high-efficiency waterproof LED with long life, high brightness and pure color.

4. Applicable to 3D modeling lights, Internet celebrity halls, KTV decorations, supermarket 3D screens, hotel decorations.

5. Small size, light weight, exquisite appearance, suitable for indoor and outdoor use